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Questions and Answers (Q&A) Information session TR2021 on 23 March 2021 
 
1. A question about message definitions (for Jan de Jong 10:40h): besides the xsd, sample xml and Word documents, will market participants also receive the WSDL for generating and validating XML documents? Reason for this question: I have not yet received the WSDL for message definitions, and this WSDL has thus far always been part of the EDSN message definitions. (Johan vt Land, Joulz Meetbedrijf) 
Answer: A description about using WSDL in message definitions for the MMC Hub has been provided in: technical guide - Measurements & Allocations Documents. This technical guide can be found on myTennet:
https://my.tennet.eu/nl/Paginas/ITConnectivity.aspx#/mmchub/webservices

It is called Measurements Allocations - Technical Guide. It states that the documents below are also needed:
· VolumeSeries-wsdl
· VolumeInstallationSeries-wsdl
· mmchub-VolumeSeries-wsdl
· mmchub-VolumeInstallationSeries-wsdl
· mmchub-MeasurementSeries-wsdl
· mmchub-MeasurementSeriesRevision-wsdl
· mmchub-AllocationVolumeRevision-wsdl
· MeasurementSeries-wsdl
· MeasurementSeriesRevision-wsdl
· AllocationVolumeRevision-wsdl


2. What if a BRP receives metering data but does not expect it?
Answer: If a BRP receives metering data for a connection where the concerned BRP is not registered, then the BRP is able to reject the message with error code 656: The BRP is not registered as BRP for the connection.

3. Exchange metering data time series. Edine messages currently only contain Electricity metering data. Will we now also be receiving them for Gas via the Tennet MMC Hub?
Answer: Yes. 

4. For Gas, the Ball messages will only be sent to the SUP; is this in scope?
Answer: Not in scope for TR2021. They will continue to be sent via the Nexus Hub. 



5. The reason mentioned in the revision example was that the estimated repair method was too long. This is not an origin indicator for time series in the service description BS Uitwisselen meetgegevens tijdseries, or does this refer to a calculated indication? And must the calculated value for a PAP (serial MLOEA) be passed on as metered?
Answer: The recipient should personally infer this using the metering days he has received over the past few days. The metering responsible party knows where a metering device is located, and thus what he meters directly. And that which he does not meter directly, but has derived, can be supplied as metered. 

6. The messages stated that certain things were optional. How will the grid operator indicate this? How will MRP’s know which data is expected of them?
Answer: mandatory and optional fields have been defined in the XML diagram. This is specific for each role. This has been specified in the service messages. 
Exchange metering data and metre readings. The MRP supplies volumes and meter readings to the BRP and DSO. The MRP also provides residual volumes for gas and (weekly/monthly) peak load for the DSO alone. This data has thus been defined as optional in the XML messages and also been described as such in this service description.

7. To what extent can Allocatie 2.0 be expected to have an impact on the process carried out by SUP parties prior to this, namely forecasting?
Due to the objective of removing barriers in the interest of the energy transition/innovation, the risk of imbalance could increase if SUP parties do not prepare in good time.
We have already witnessed this on a small scale at iSMA, whereby SUP parties think they are not at risk if they charge customers at the (regular) market price, while their forecasting has no idea about the profile of the customers in question.
We look forward to your response.
Answer: All market roles are represented in the NEDU Programme Allocatie 2.0. We assume that representatives of the various market roles will inform their members about this impact on suppliers.

8. Have agreements already been made about the testing dates and period for function tests?
Answer: No specific agreements have been made in this regard.

9. Is it possible to appoint a 'promoter' per group?
Answer: the GAT detailed testing plan will be presented for confirmation in September. This will be part of the GAT. This is also when the composition of GAT test groups will be announced on mijnNEDU.

10. Will testing and qualification take place per market participant or per back-end (I am referring to C-ARM, where all DSO's use the same system to generate their messages)?
Answer: Testing will take place per market participant. When doing so, it is easier if one common system is used. 

11. Will test cases also be taken into account during the switch between summer/winter and winter/summer time?
Answer: They will be taken into account.

12. myTennet (Pages - IT Connections (tennet.eu)) currently features no wsdl files. What is the time frame for publishing them?
Answer: They are now available.
https://my.tennet.eu/nl/Paginas/ITConnectivity.aspx#/mmchub/webservices

13. Where can I find the BRS 3.0?
Answer: BRS can be found on mijnNEDU under ‘releases/theme release TR2021’ because it is still part of an ongoing project. 
Theme Release 2021 - Documents - All documents (sharepoint.com)

14. Is it possible to compile a one pager about the purpose and composition of KBG-T? 
Answer: this will be compiled and then published on mijnNEDU. 

15. Is MaandMax Invoeding (MonthlyMax Input) compulsory for MRP and has the means for determining MaandMax Invoeding been determined?
Answer: It is not compulsory to supply the MaandMax Invoeding. A NEDU issue still needs to be compiled in order to incorporate this obligation into the codes. In anticipation of this obligation, the information can be exchanged via the new messages. This means the message is future-proof and does not have to be modified later down the line.
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